****

**TEST APPLICATION FORM**

|  |  |  |
| --- | --- | --- |
| **Applicant Name:** |  | **Laboratory’s Use Only:** |
| Address: |  | Report No.:  Due Date |
| Contact Person: |  |
| Telephone/Cell: |  |
| E-Mail: |  | |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **If the payer is different from the applicant, please clarify:** | | | | | | | |
| **Payer Name:** |  | | | | | | |
| Address: |  | | | | | | |
| Contact Person: |  | | | | | | |
| Telephone/Cell: |  | | | | | | |
| E-Mail: |  | | | | | | |
| **Report Delivered To:**  Applicant  Payer **Invoice Delivered To:**  Applicant  Payer | | | | | | | |
| Sample Description: | |  | | | Buyer’s Name: | |  |
| Order No. | |  | | | Style Number: | |  |
| Color: | |  | | | | | |
| **Care Instruction:** | | | | Composition: |  | | |
| Agent Name: |  | | |
| Country of Destination: |  | | |
| **Test Required**  **Dimensional Stability:**  Washing:  x 1  x 3 washes  Dry cleaning  during steaming  during ironing  **Apparence:**  After washing:  x 1  x 3 washes  After dry-cleaning  **Spirality/Twisting:**  After washing:  x 1  x 3 washes  **Print Durability:**  After washing:  x 1  x 3 washes  **Colour Fastness to:**  Washing  Water  Dry cleaning  Rubbing/crocking  Perspiration  Artificial light: Grade  4  5  6  Sea water  Swimming pool water  Chlorine bleach  Saliva and perspiration  Phenolic Yellowing | | | **Physical**  Tensile strength  Tear strength  Seam slippage ISO 13936-1/2  Seam strength ISO 13935-1/2  Bursting strength  Pilling resistance  Abrasion resistance  Water repellency  Attachment strength  Moisture drying time  Thread per inch/stitch density  Yarn count  Fabric weight  Fibre composition  Zipper strength  Flammability  Stretch & Recovery (Elongation)  Care label recommendation/Verification  Odour | | | **Chemical:**  AZO dyes  pH value  Formaldehyde  Extractable heavy metals  Heavy metals (Packaging materials)  Chlorinated phenols-PCP/TECP/OPP  Allergenic & Carcinogenic dyes  Phthalates  Organic tin compounds  Chlorinated benzenes and toluene  AP/APEO  PFC  PAH  Release of Nickel  Total Cadmium  Total Lead  VOC  PVC Identification  DMFu  SCCP / MCCP  **Test Package:**  PPC  Oeko-Tex Standard 100, Appendix 4  Oeko-Tex Standard 100, Appendix 6 | |
| **Others:** | | | | | | | |

**Service Type:**  Regular (04 Working Days)  Express (03 Working Days, 40% Surcharge)  Emergency (02 Working Days, 100% Surcharge)

Same Day (12 Hours, 150% Surcharge)

**Note: Special service is applicable only for selective test. Nickel release test takes 9-10 days by its nature of testing.**

We request for the above tests and agree that all testing will be carried out subject to **Hohenstein Laboratories Bangladesh Limited** scale of charges as set forth in their price list of which we have seen a copy.

Date:Authorized Signature and Company Chop**:**

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_